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NP SERIES 12V
Valve Regulated Lead Acid (VRLA) Batteries
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· Non – Spillable
· Sealed and Maintenance-Free Battery
· High Quality and High Reliability
· Absorbent Glass Matt (AGM) Technology
· 13.5V to 13.8V Standby Voltage
· Computer - Aided Design and Manufacturing
· CE Approved
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	Model
	Nominal Voltage
	Rated Capacity
	Approx. Dimension
（mm）
	
Terminal 
type

	
	
	
	Length
	Width
	Height
	

	
	
	
	±3
	±3
	±3
	

	NP12-7AH
	12VDC
	7AH
	151
	65
	95
	T1/T2

	NP12-9AH
	12VDC
	9AH
	151
	65
	95
	T1/T2

	NP12-12AH
	12VDC
	12AH
	151
	98
	95
	T1/T2

	NP12-18AH
	12VDC
	18AH
	181
	77
	167
	T3/T12

	NP12-26AH
	12VDC
	26AH
	166
	175
	125
	T4/T12

	NP12-40AH
	12VDC
	40AH
	197
	165
	170
	T14

	NP12-55AH
	12VDC
	50AH
	230
	138
	211
	T14

	NP12-65AH
	12VDC
	65AH
	350
	166
	179
	T14

	NP12-80AH
	12VDC
	80AH
	260
	169
	211
	T14

	NP12-90AH
	12VDC
	90AH
	306
	169
	211
	T14

	NP12-100AH
	12VDC
	100AH
	330
	171
	214
	T16

	NP12-120AH
	12VDC
	120AH
	409
	176
	225
	T16

	NP12-150AH
	12VDC
	150AH
	485
	172
	240
	T16

	NP12-200AH
	12VDC
	200AH
	522
	238
	218
	T18

	NP12-250AH
	12VDC
	250AH
	521
	269
	220
	T18
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AUTOMATION SPECIALISTS AND POWER EXPONENTS, INC.
ASPEX Bldg., 159 Boni Avenue, Brgy. Plainview, Mandaluyong City
Trunk line: (02) 8997-0000   Fax: (02) 8532-7228
www.aspexinc.com.ph
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